Eq. Run hrs/ day
Check abnormality in Ambient air like Bad odor / Heavy dust / Any Chemical handling
Check control cabinet / SFC cabinet / cooler filter mats, clean / replace if necessary
Check / Clean cooler check fan blades and guarding
Check coupling / belt tension, tight if necessary
Check / change the Air filter	Dp	bar
Check / change the Oil filter
Check / change Oil separater	Dp	bar, Temp
Check / change the Oil	Oil Level
Check / Air filter cap, Suction hose for any leak or crack / damage
Check / change the Valve kits
Check bearing lubrication M.Motor	Fan Motor	regrease if necessary
Check electrical connection and tight if necessary
Check overcurrent relays, switches M.Motor	A, Fan Motor	A, Controller	A
Check Voltage : L1	V, L2	V, L3	V, Trans Vol	V, VDc
Check current consumption (Load): U1 A, V1	A, W1 A	rpm
Check current consumption (Idle): Ul A, V1	A, W1 A	rpm
Check Air Cooler Fan motor current : U1	A, V1 A, VV1	A	rpm
Check Oil Cooler Fan motor current : U1	A, V1 A, W1	A	rpm
Room Temp	C, ADT : 	C PD temp •	C Motor Temp	C
Pre. Set SP	bar, SD	bar, P.idle	bar,
Pre Set Pin	bar, Psys	bar,
Check door and guard interlocks and emergency stop function
Check all sensor tight connections and register if any safety device bypassed
Check for any Air / Oil Leakages in the compressor
Check and maintain Eco drain Valve
Duty Cycle Total	 Duty Cycle Dt	 Since	%
Check Message Histroy Since ___ if any Unusal Alarms or Warrnings
Check / Clean Air dryer condensor & Fan Molar Direction
Check condensate drain function
Check refrigerant circuit and Air Circuit for leaks
Check current consumbtion : Line U1 A V1 A VV1 A
Check Voltage : L.11 	V, V1 V, W1 V
Check protection switchesRef Comp.	Fan Motor
Check Ps	bar, Pc 	bar :
PS Dew Point : [ ] Blue, [ ] Green. [ ] Red 	C
Check Auto On/Off operation [ ] : Switching on	C, Switching Off	C
Check Message Histroy if any Unusal
Check / Replace Air treatment filter cartridge	Dp	Bar
Check Filter Condensate drain function
Start of Work
End of Work
Travel Time
Travel Km
Guidelines For Performance Improvement Work Remarks
Customer Remark


Altered
--------
Check abnormality in Ambient air like Bad odor / Heavy dust / Any Chemical handling
Check control cabinet / SFC cabinet / cooler filter mats, clean / replace if necessary
Check / Clean cooler check fan blades and guarding
Check coupling / belt tension, tight if necessary
Check / change the Air filter	Dp	bar
Check / change the Oil filter
Check / change Oil separater	Dp	bar, Temp
Check / change the Oil	Oil Level
Check / Air filter cap, Suction hose for any leak or crack / damage
Check / change the Valve kits
Check bearing lubrication M.Motor	Fan Motor	regrease if necessary
Check electrical connection and tight if necessary

Check overcurrent relays, switches M.Motor	A
Check overcurrent relays, switches Fan Motor	A
Check overcurrent relays, switches Controller	A

Check Voltage : L1	V,
Check Voltage : L2	V,
Check Voltage : L3	V,
Check Voltage : Trans Vol	V, VDc

Check current consumption (Load): U1	A
Check current consumption (Load): V1	A
Check current consumption (Load): W1	A	rpm

Check current consumption (Idle): Ul	A
Check current consumption (Idle): V1	A
Check current consumption (Idle): W1	A	rpm

Check Air Cooler Fan motor current : U1	A
Check Air Cooler Fan motor current : V1	A
Check Air Cooler Fan motor current : VV1	A	rpm

Check Oil Cooler Fan motor current : U1	A
Check Oil Cooler Fan motor current : V1	A
Check Oil Cooler Fan motor current : W1	A	rpm



Room temp •	C, ADT : 	C PD temp •	C Motor Temp	C
Pre. Set SP	bar, SD	bar, P.idle	bar, Pin	bar, Psys	bar,
Check door and guard interlocks and emergency stop function
Check all sensor tight connections and register if any safety device bypassed
Check for any Air / Oil Leakages in the compressor
Check and maintain Eco drain Valve
Duty Cycle Total	 Duty Cycle Dt	 Since	%
Check Message Histroy Since 	. if any Unusal Alarms or Warrnings
Check / Clean Air dryer condensor & Fan Molar Direction
Check condensate drain function
Check refrigerant circuit and Air Circuit for leaks

Check current consumbtion : Line U1
Check current consumbtion : A V1
Check current consumbtion : A VV1 	A

Check Voltage : L.11 	V
Check Voltage : V1 	V
Check Voltage : W1 	V


Check protection switchesRef Comp.	Fan Motor


Check Ps	bar Check Pc 	bar
Check Dew Point : Blue, Green, Red

Check Auto On/Off operation - Switching on	C
Check Auto On/Off operation - Switching Off	C

Check Message Histroy if any Unusal
Check / Replace Air treatment filter cartridge	Dp	Bar
Check Filter Condensate drain function

